**HOW TO SPECIFY**

**Model RNS**

**STEEL STAMPED SQUARE CEILING DIFFUSER**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model RNS Stamped Square Ceiling Diffusers** of the sizes and capacities as shown on the plans and air distribution schedules. The diffuser shall be manufactured from corrosion-resistant steel and have four concentric cones in all sizes, except the 20" x 20" (500 x 500) module size which will consist of three cones. The inner cone assembly is to be removable using a spring clip arrangement that permits quick, easy installation and removal. The diffuser shall have a removable plug for screwdriver adjustment of the optional damper without removing the inner core. The finish shall be AW Appliance White (optional finishes are available).The manufacturer shall provide published performance data for the diffuser, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2006. |

**Model ARNS**

**ALUMINUM STAMPED SQUARE CEILING DIFFUSER**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model ARNS Stamped Square Ceiling Diffusers** of the sizes and capacities as shown on the plans and air distribution schedules. The diffuser shall have four die-formed aluminum concentric cones in all sizes, except the 20" x 20" (500 x 500) module size which will consist of three cones. The inner cone assembly is to be removable using a spring clip arrangement that permits quick, easy installation and removal. The diffuser shall have a removable plug for screwdriver adjustment of the optional damper without removing the inner core. The finish shall be AW Appliance White (optional finishes are available).The manufacturer shall provide published performance data for the diffuser, which shall be tested in accordance with ANSI/ASHRAEStandard 70-2006. |

**Model RNS3 AND ARNS3**

**STAMPED SQUARE CEILING DIFFUSER – 3 CONE**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model** (select one) **RNS3** (steel) or **ARNS3** (aluminum) **Stamped Square Ceiling Diffusers** of the sizes and capacities as shown on the plans and air distribution schedules. Model RNS3 shall be manufactured from corrosion-resistant steel and have three die-formed concentric cones in all sizes. Model ARNS3 shall be manufactured from aluminum with corrosion- resistant steel bracketry. The inner cone assembly is to be non-removable. The diffuser shall have a removable plug for screwdriver adjustment of the optional damper without removing the inner core. The finish shall be AW Appliance White (optional finishes are available).The manufacturer shall provide published performance data for the diffuser, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2006. |

**Model RNS2**

**STAMPED SQUARE CEILING DIFFUSER – 2 CONE**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model RNS2 Stamped Square Ceiling Diffusers** of the sizes and capacities as shown on the plans and air distribution schedules. The diffuser shall be manufactured from corrosion-resistant steel and incorporate two die-formed concentric cones. The diffuser shall have a removable plug for screwdriver adjustment of the optional damper without removing the inner core. The finish shall be AW Appliance White (optional finishes are available).The manufacturer shall provide published performance data for the diffuser, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2006. |