**HOW TO SPECIFY**

**Models 5130H-HD(-O), 5130V-HD(-O), 51FH-HD(-O), 51FV-HD(-O)**

**ALUMINUM HEAVY DUTY BAR RETURN GRILLES AND REGISTERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model** (select one) **5130H-HD, 5130V-HD, 51FH-HD** or **51FV-HD Aluminum Heavy Duty Bar Return Grilles** of the type and size as shown on the plans and air distribution schedules. The grille shall have extruded aluminum reinforced fixed blades and welded frame with reinforced mitered corners. The finish shall be AW Appliance White (optional finishes are available).(Optional) An opposed blade damper, constructed of heavy gauge corrosion-resistant steel (aluminum is optional) and operable from the face of the grille, shall be provided with all units.The manufacturer sh ll provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |