**HOW TO SPECIFY**

**Models 5145H(-O), 5145V(-O), 5155H(-O), 5155V(-O), 51FH(-O), 51FV(-O)**

**ALUMINUM RETURN GRILLES AND REGISTERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model** (select one) **5145H, 5145V, 5155H, 5155V, 51FH** or **51FV Return Grilles** of the types and sizes as shown on the plans and air distribution schedules. The grilles shall have extruded aluminum fixed blades and extruded aluminum frames that have reinforced mitered corners. The finish shall be AW Appliance White (optional finishes are available).(Optional) An opposed blade damper constructed of heavy gauge corrosion-resistant steel (aluminum is optional) and operable from the face of the grille, shall be provided with all units.The manufacturer shall provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |

**Models 6145H(-O), 6145V(-O), 6155H(-O), 6155V(-O), 61FH(-O), 61FV(-O)**

**STEEL RETURN GRILLES AND REGISTERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model** (select one) **6145H, 6145V, 6155H, 6155V, 61FH** or **61FV Return Grilles** of the types and sizes as shown on the plans and air distribution schedules. The grilles shall have roll-formed corrosion-resistant steel fixed blades and the frame is to be constructed from roll-formed corrosion-resistant steel and have reinforced mitered corners. The finish shall be AW Appliance White (optional finishes are available).(Optional) An opposed blade damper, constructed of heavy gauge corrosion-resistant steel and operable from the face of the grille, shall be provided with all units.The manufacturer shall provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |

**Models 6745H(-O), 6745V(-O), 6755H(-O), 6755V(-O), 67FH(-O), 67FV(-O)**

**STAINLESS STEEL RETURN GRILLES AND REGISTERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model** (select one) **6745H, 6745V, 6755H, 6755V, 67FH** or **67FV Return Grilles** of the types and sizes as shown on the plans and air distribution schedules. The grilles shall be constructed entirely from 304 stainless steel (316 optional) and have a single set of streamlined shaped roll-formed fixed blades. The frames shall be constructed of heavy gauge stainless steel and have reinforced mitered corners. All exposed surfaces shall have a #4 Brushed Satin Polished finish (optional finish is AW Appliance White).(Optional) A stainless steel opposed blade damper, adjustable from the face of the grille, shall be provided with all units.The manufacturer shall provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |