**HOW TO SPECIFY**

**Models 4260, 4260AA**

**EGGCRATE RETURN CEILING DIFFUSERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**  Furnish and install **Nailor Model** (select one) **4260** (corrosion-resistant steel frame/backpan) or **4260AA** (aluminum frame/backpan) **Eggcrate Return Ceiling Diffusers** of the sizes and capacities as shown on the plans and air distribution schedules. The diffuser shall have a removable aluminum grid core that is 1/2" x 1/2" x 1/2" (13 x 13 x 13) and extends the full face of the diffuser. The finish shall be AW Appliance White (optional finishes are available).  The manufacturer shall provide published performance data for the diffuser, which shall be tested in accordance with ANSI/ASHRAE  Standard 70 – 2006. |