**HOW TO SPECIFY**

**Model TWR**

**“TWISTER” STAMPED SQUARE CEILING SWIRL DIFFUSER**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model TWR 'Twister' Ceiling Swirl Diffusers** of the sizes and capacities as shown on the plans and air distribution schedules. The diffuser shall be manufactured from heavy gauge corrosion-resistant steel. Radial induction vanes shall be one-piece stamped construction. The diffuser is to be sizes to suit a 24" x 24" (600 x 600) ceiling suspension system. The round duct connection collar shall be an integral part of the diffuser assembly and be not less than 1 1/4" (32) high. The diffuser shall have a removable plug for screwdriver adjustment of the optional damper without removing the inner core. The finish shall be AW Appliance White (optional finishes are available).The manufacturer shall provide published performance data for the diffuser, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2006. |