**HOW TO SPECIFY**

**Models 51RC(-O), 51RCD(-O)**

**REVERSIBLE CORE GRILLES AND REGISTERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model** (select one) **51RC** or **51RCD (with rear vanes) Reversible Core Grilles** of the types and sizes as shown on the plans and air distribution schedules. The grille shall have extruded aluminum blades and frame. The blade core is to be removable and may be rotated or reversed to achieve any one of four air deflection patterns. The finish shall be AW Appliance White (optional finishes are available).(Optional) An opposed blade damper, constructed of heavy gauge corrosion-resistant steel (aluminum is optional) and operable from the face of the grille, shall be provided with all units.The manufacturer shall provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |