**HOW TO SPECIFY**

**Models 71DV(-O), 71DH(-O)**

**AIRFOIL BLADE SUPPLY GRILLES AND REGISTERS – DOUBLE DEFLECTION**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**  **71DV, 71DH Double Deflection**  Furnish and install **Nailor Model** (select one) **71DV** or **71DH Airfoil Blade Double Deflection Supply Grilles** of the types and sizes as shown on the plans and air distribution schedules. The grilles shall have a double set of extruded aluminum adjustable blades that are airfoil shaped and spaced on 3/4" (19) centers. The frame is to be constructed from heavy gauge extruded aluminum with reinforced mitered corners. The finish shall be AW Appliance White (optional finishes are available).  (Optional) An opposed blade damper, constructed of heavy gauge corrosion-resistant steel (aluminum is optional) and operable from the face of the grille, shall be provided with all units.  The manufacturer shall provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |

**Models 71SV(-O), 71SH(-O)**

**AIRFOIL BLADE SUPPLY GRILLES AND REGISTERS – SINGLE DEFLECTION**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**  Furnish and install **Nailor Model** (select one) **71SV** or **71SH Airfoil Blade Single Deflection Supply Grilles** of the types and sizes as shown on the plans and air distribution schedules. The grilles shall have a single set of extruded aluminum adjustable blades that are airfoil shaped and spaced on 3/4" (19) centers. The frame is to be constructed from heavy gauge extruded aluminum with reinforced mitered corners. The finish shall be AW Appliance White (optional finishes are available).  (Optional) An opposed blade damper, constructed of heavy gauge corrosion-resistant steel (aluminum is optional) and operable from the face of the grille, shall be provided with all units.  The manufacturer shall provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |