**HOW TO SPECIFY**

**Models 45DL1(-O), 45DL2(-O), 45DLC1, 45DLC2**

**DRUM LOUVERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model** (select one) **45DLC1** or **45DLC2 Spiral Duct Drum Louvers** or **Nailor Model** (select one) **45DL1** or **45DL2 Drum Louvers** of the types and sizes as shown on the plans and air distribution schedules. The louver is to be manufactured from extruded aluminum and have a cylindrical adjustable drum that rotates. The blades are to have a paddle like profile that pivot on nylon bushings. A perimeter gasket is to be included around the frame and a felt seal is to be around the drum. The finish shall be AW Appliance White (optional finishes are available).(Optional) An opposed blade damper, constructed of heavy gauge corrosion-resistant steel and operable from the face of the grille, shall be provided with all units.The manufacturer shall provide published performance data for the louver, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |