**HOW TO SPECIFY**

**Models 6755H-HD(-O), 6755V-HD(-O)**

**STAINLESS STEEL HEAVY DUTY BAR RETURN GRILLES AND REGISTERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**Furnish and install **Nailor Model** (select one) **6755H-HD** or **6755V-HD Stainless Steel Heavy Duty Return Grilles** of the types and sizes as shown on the plans and air distribution schedules. The grilles shall be constructed entirely from 304 stainless steel (316 optional) with welded and reinforced frames. The blades shall be fixed at 45°, spaced on 1/2" (13) centers, and shall be reinforced by a support mullion on maximum 8" (203) centers. All exposed surfaces shall have a #4 Brushed Satin Polished finish (optional finish is AW Appliance White).(Optional) A stainless steel opposed blade damper, adjustable from the face of the grille, shall be provided with all units.The manufacturer shall provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |