**HOW TO SPECIFY**

**Models 6145H-HD(-O), 6145V-HD(-O), 61FH-HD(-O), 61FV-HD(-O)**

**STEEL HEAVY DUTY BAR RETURN GRILLES AND REGISTERS**

|  |
| --- |
| **SUGGESTED SPECIFICATION:**  Furnish and install **Nailor Model** (select one) **6145H-HD, 6145V-HD, 61FH-HD** or **61FV-HD Steel Heavy Duty Return Grilles** of the types and sizes as shown on the plans and air distribution schedules. The grilles shall have fixed 14 gauge steel blades spaced on 1/2" (13) centers and a heavy duty 16 gauge steel welded frame. The finish shall be AW Appliance White (optional finishes are available).  (Optional) An opposed blade damper, constructed of heavy gauge corrosion-resistant steel and operable from the face of the grille, shall be provided with all units.  The manufacturer shall provide published performance data for the grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70 – 2006. |